EZ100PU Driver v1.4.0 Installation guild for Linux:

   For installing EZ100PU PC/SC driver, please follow these steps -

   1. Install the packages of pcsc-lite v0.9 or higher (Recommanded 1.1.1 or 1.2.9). 
      You can find this package from our attached or from http://www.linuxnet.com/middle.html.
	To install pcsc-lite, execute this command-
			rpm -ivh pcsc-lite-1.1.1-1-redhat.i386.rpm

   2. Execute installation program : ./install
      
   3. Reboot the system.

   4. After reboot, insert a card. If the led of the reader turns red, the installation 
      of EZ100PU driver is successful.

   Notice: 1. The recommaned version of kernel is 2.4 or higher.
           2. If you have installed EZ100PU driver v1.3.4 or lower, please reinstall it first 
              before executing "install" program.
	      To uninstall v1.3.4 or lower, remove the settings of EZ100PU driver in the 
              /etc/reader.conf.


